**Supplementary Information**

**On**

**Theoretical and Experimental Analysis of Miniaturization of Conventional Oscillatory Flow Technology**

Kirubanandan Shanmugam1, 2

1. Former Master of Applied Science (MASc) Student, Chemical Engineering Division, Department of Process Engineering and Applied Science, Dalhousie University, Sexton Campus, Halifax, NS, Canada.
2. Department of Biotechnology, Sree Sastha Institute of Engineering and Technology (Affiliated to Anna University, Chennai, India), Chembarabakkam, Chennai – 600123, India.

**Pump Curve – Experimental Data**

S1. Pressure drop vs. Volumetric flow rate

S2. Pressure drop vs. volumetric flow rate

S3. Pressure drop vs. Volumetric flow rate

**Valve Positioning:**

**The change in the position of the valve can be rearranged as per the**

**Future work**

The preliminary feasibility of OFT in minichannels has been investigated and theoretical analysis suggests that the OFT in minichannel showed increase Nusselt numbers at equivalent energy dissipation relative to a smooth pipe at reduced dimensions. The design of mini-fluidic channels specifically for oscillatory flow will be performed and tested experimentally to evaluate momentum, heat and mass transfer performance relative to both a smooth pipe, and more recent minifluidic contacting devices.

C:\Users\Adam\Documents\Funding\CFI\Sketches\Exported 2d images\A5 Reactor blow-up and combined.tif

Figure 1 –Modular Fluidic Platform

Fluidic platform integrated with high-resolution rapid prototyping capabilities to construct and test new geometries. It is Capable of 3D prints with 20-100 μm practical resolution. This plate and frame mini-fluidic arrangements is suitable for scale up the chemical processing. These modules can be arranged like plate – frame filter press for large scale production of chemical in mini-fluidics approach (Norbert Kockmann, 2011). [27]